T2420 116:021 SEGGER J-Link V6.46 Log File (0000ms, 22969ms total)
T2420 116:021 DLL Compiled: May 23 2019 17:49:56 (0000ms, 22969ms total)
T2420 116:021 Logging started @ 2024-09-13 14:00 (0000ms, 22969ms total)
T2420 116:021 JLINK_SetWarnOutHandler(...) (0000ms, 22969ms total)
T2420 116:021 JLINK_OpenEx(...)
Firmware: J-Link V9 compiled May  7 2021 16:26:12
Hardware: V9.60
S/N: 69665339
Feature(s): RDI, GDB, FlashDL, FlashBP, JFlash
TELNET listener socket opened on port 19021Device "STM32F103C8" selected.WEBSRV 
Starting webserver (0029ms, 22998ms total)
T2420 116:021 WEBSRV Webserver running on local port 19080 (0030ms, 22999ms total)
T2420 116:021   returns O.K. (0030ms, 22999ms total)
T2420 116:051 JLINK_GetEmuCaps()  returns 0xB9FF7BBF (0000ms, 22999ms total)
T2420 116:051 JLINK_TIF_GetAvailable(...) (0000ms, 22999ms total)
T2420 116:051 JLINK_SetErrorOutHandler(...) (0000ms, 22999ms total)
T2420 116:051 JLINK_ExecCommand("ProjectFile = "C:\Users\soft-001\Desktop\CH32F103C8T6\CH32F103EVT\EVT\EXAM\USB\USBD\CH372\JLinkSettings.ini"", ...). Device "STM32F103C8" selected.  returns 0x00 (0001ms, 23000ms total)
T2420 116:052 JLINK_ExecCommand("Device = CH32F103R8", ...). Device "STM32F103C8" selected.  returns 0x00 (0000ms, 23000ms total)
T2420 116:052 JLINK_ExecCommand("DisableConnectionTimeout", ...).   returns 0x01 (0000ms, 23000ms total)
T2420 116:052 JLINK_GetHardwareVersion()  returns 0x17700 (0000ms, 23000ms total)
T2420 116:052 JLINK_GetDLLVersion()  returns 64600 (0001ms, 23001ms total)
T2420 116:053 JLINK_GetFirmwareString(...) (0000ms, 23001ms total)
T2420 116:053 JLINK_GetDLLVersion()  returns 64600 (0000ms, 23001ms total)
T2420 116:053 JLINK_GetCompileDateTime() (0000ms, 23001ms total)
T2420 116:053 JLINK_GetFirmwareString(...) (0000ms, 23001ms total)
T2420 116:053 JLINK_GetHardwareVersion()  returns 0x17700 (0000ms, 23001ms total)
T2420 116:053 JLINK_TIF_Select(JLINKARM_TIF_SWD)  returns 0x00 (0000ms, 23001ms total)
T2420 116:053 JLINK_SetSpeed(50) (0000ms, 23001ms total)
T2420 116:053 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)  returns JLINKARM_RESET_TYPE_NORMAL (0000ms, 23001ms total)
T2420 116:053 JLINK_Reset() >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>STM32 (connect): Can not attach to CPU. Trying connect under reset. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>
  ***** Error: STM32: Connecting to CPU via connect under reset failed. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>STM32 (connect): Can not attach to CPU. Trying connect under reset. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>
  ***** Error: STM32: Connecting to CPU via connect under reset failed.
JLINK_GetId() >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>STM32 (connect): Can not attach to CPU. Trying connect under reset. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>
  ***** Error: STM32: Connecting to CPU via connect under reset failed. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>STM32 (connect): Can not attach to CPU. Trying connect under reset. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>
  ***** Error: STM32: Connecting to CPU via connect under reset failed.  returns 0x00000000
 (0772ms, 24548ms total)
T2420 117:600 JLINK_GetId() >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>STM32 (connect): Can not attach to CPU. Trying connect under reset. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>
  ***** Error: STM32: Connecting to CPU via connect under reset failed. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>STM32 (connect): Can not attach to CPU. Trying connect under reset. >0x10B TIF> >0x10F TIF> >0x10B TIF> >0x10F TIF>
  ***** Error: STM32: Connecting to CPU via connect under reset failed.
  returns 0x00000000 (0776ms, 25324ms total)
T2420 118:377 JLINK_GetFirmwareString(...) (0000ms, 25324ms total)
T2420 274:340 JLINK_Close() (0006ms, 25330ms total)
T2420 274:340  (0006ms, 25330ms total)
T2420 274:340 Closed (0006ms, 25330ms total)
